|  |  |
| --- | --- |
| **Rancher Special Platform Specifications** | |
| Sizes: | 8’3” x 84” – 92” – 96”, 9’4" x 92” – 96” – 99 ½”, 10’, 11’4", 12’ x 96”  or 99 1/2”  96” & 99 ½” wide bodies are tapered at front for sleek style and appearance. Square front optional |
| Floor: | Treadplate, 12 gauge |
| Side Rail: | 7” vertical face |
| Pockets: | 3/16” formed steel to accommodate 2” x 4” lumber |
| Tie Rail: | 3/8” x 2” steel segmented for ease in fuel fill installation |
| Crossmembers: | 3” 4.1# structural channel |
| Longsills: | 6” 8.2# |
| Headboard: | 14 gauge smooth steel panel with 3” x 2” – 11 gauge rectangular tubing frame with louvered window: 39” hight; 35” high on 8’3” x 84” |
| Rear Apron: | 3/16” smooth steel |
| Gooseneck Hitch: | Recessed gooseneck hitch with safety chain loop standard.  (ball not included) Atwood B-25 retractable ball assembly optional. |
| Receiver Hitch: | 3” x 4” x ¼” rectangular tubing frame with tube for 2” receiver hitch;  safety chain loops; and tail light brackets. |
| Lights: | Required lighting & marking per FMVSS108 installed |
| Standard finish for platforms in black. | |